| CMSIS-RTOS2 Real-Time Operating System API |

Loading...
Searching...
No Matches
Data Structures | Functions
Message Queue
CMSIS-RTOS2 API

Exchange messages between threads in a FIFO-like operation. More...

## Data Structures
struct | osMessageQueueAttr_t
| Attributes structure for message queue. More...

## Functions
osMessageQueueId_t | osMessageQueueNew (uint32_t msg_count, uint32_t msg_size, const osMessageQueueAttr_t *attr)
| Create and Initialize a Message Queue object.
const char * | osMessageQueueGetName (osMessageQueueId_t mq_id)
| Get name of a Message Queue object.
osStatus_t | osMessageQueuePut (osMessageQueueId_t mq_id, const void *msg_ptr, uint8_t msg_prio, uint32_t timeout)
| Put a Message into a Queue or timeout if Queue is full.
osStatus_t | osMessageQueueGet (osMessageQueueId_t mq_id, void *msg_ptr, uint8_t *msg_prio, uint32_t timeout)
| Get a Message from a Queue or timeout if Queue is empty.
uint32_t | osMessageQueueGetCapacity (osMessageQueueId_t mq_id)
| Get maximum number of messages in a Message Queue.
uint32_t | osMessageQueueGetMsgSize (osMessageQueueId_t mq_id)
| Get maximum message size in a Message Queue.
uint32_t | osMessageQueueGetCount (osMessageQueueId_t mq_id)
| Get number of queued messages in a Message Queue.
uint32_t | osMessageQueueGetSpace (osMessageQueueId_t mq_id)
| Get number of available slots for messages in a Message Queue.
osStatus_t | osMessageQueueReset (osMessageQueueId_t mq_id)
| Reset a Message Queue to initial empty state.
osStatus_t | osMessageQueueDelete (osMessageQueueId_t mq_id)
| Delete a Message Queue object.

## Description

Exchange messages between threads in a FIFO-like operation.

Message passing is another basic communication model between threads. In the message passing model, one thread sends data explicitly, while another thread receives it. The operation is more like some kind of I/O rather than a direct access to information to be shared. In CMSIS-RTOS, this mechanism is called s message queue. The data is passed from one thread to another in a FIFO-like operation. Using message queue functions, you can control, send, receive, or wait for messages. The data to be passed can be of integer or pointer type:

CMSIS-RTOS Message Queue

Compared to a Memory Pool, message queues are less efficient in general, but solve a broader range of problems. Sometimes, threads do not have a common address space or the use of shared memory raises problems, such as mutual exclusion.

Note
  The functions osMessageQueuePut, osMessageQueueGet, osMessageQueueGetCapacity, osMessageQueueGetMsgSize, osMessageQueueGetCount, osMessageQueueGetSpace can be called from Interrupt Service Routines.

## Data Structure Documentation

## ◆ osMessageQueueAttr_t

struct osMessageQueueAttr_t

Attributes structure for message queue.

Specifies the following attributes for the osMessageQueueNew function.

Data Fields
const char * | name | name of the message queue Pointer to a constant string with a human readable name (displayed during debugging) of the message queue object. Default: NULL no name specified.
uint32_t | attr_bits | attribute bits Reserved for future use (must be set to '0' for future compatibility).
void * | cb_mem | memory for control block Pointer to a memory for the message queue control block object. Refer to Manual User-defined Allocation for more information. Default: NULL to use Automatic Dynamic Allocation for the message queue control block.
uint32_t | cb_size | size of provided memory for control block The size (in bytes) of memory block passed with cb_mem. Required value depends on the underlying kernel implementation. Default: 0 as the default is no memory provided with cb_mem.
void * | mq_mem | memory for data storage Pointer to a memory for the message queue data. Refer to Manual User-defined Allocation for more information. Default: NULL to use Automatic Dynamic Allocation for the memory pool data.
uint32_t | mq_size | size of provided memory for data storage The size (in bytes) of memory block passed with mq_mem. The minimum memory block size is `msg_count * msg_size` (parameters of the osMessageQueueNew function). The msg_size is rounded up to a double even number to ensure 32-bit alignment of the memory blocks. Default: 0 as the default is no memory provided with mq_mem.

## Function Documentation

## ◆ osMessageQueueNew()

osMessageQueueId_t osMessageQueueNew | ( | uint32_t | msg_count,
|  | uint32_t | msg_size,
|  | const osMessageQueueAttr_t * | attr
| ) |  |

Create and Initialize a Message Queue object.

Parameters

  [in] | msg_count | maximum number of messages in queue.
  [in] | msg_size | maximum message size in bytes.
  [in] | attr | message queue attributes; NULL: default values.

Returns
  message queue ID for reference by other functions or NULL in case of error.

The function osMessageQueueNew creates and initializes a message queue object. The function returns a message queue object identifier or NULL in case of an error.

The function can be called after kernel initialization with osKernelInitialize. It is possible to create message queue objects before the RTOS kernel is started with osKernelStart.

The total amount of memory required for the message queue data is at least `msg_count * msg_size`. The msg_size is rounded up to a double even number to ensure 32-bit alignment of the memory blocks.

The memory blocks allocated from the message queue have a fixed size defined with the parameter `msg_size`.

Note
  This function cannot be called from Interrupt Service Routines.

Code Example

Refer to osMessageQueuePut

## ◆ osMessageQueueGetName()

const char * osMessageQueueGetName | ( | osMessageQueueId_t | mq_id | ) |

Get name of a Message Queue object.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.

Returns
  name as null-terminated string.

The function osMessageQueueGetName returns the pointer to the name string of the message queue identified by parameter mq_id or NULL in case of an error.

Note
  This function may be called from Interrupt Service Routines.

## ◆ osMessageQueuePut()

osStatus_t osMessageQueuePut | ( | osMessageQueueId_t | mq_id,
|  | const void * | msg_ptr,
|  | uint8_t | msg_prio,
|  | uint32_t | timeout
| ) |  |

Put a Message into a Queue or timeout if Queue is full.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.
  [in] | msg_ptr | pointer to buffer with message to put into a queue.
  [in] | msg_prio | message priority.
  [in] | timeout | Timeout Values or 0 in case of no time-out.

Returns
  status code that indicates the execution status of the function.

The blocking function osMessageQueuePut puts the message pointed to by msg_ptr into the the message queue specified by parameter mq_id. The parameter msg_prio is used to sort message according their priority (higher numbers indicate a higher priority) on insertion.

The parameter timeout specifies how long the system waits to put the message into the queue. While the system waits, the thread that is calling this function is put into the BLOCKED state. The parameter timeout can have the following values:

- when timeout is 0, the function returns instantly (i.e. try semantics).
- when timeout is set to osWaitForever the function will wait for an infinite time until the message is delivered (i.e. wait semantics).
- all other values specify a time in kernel ticks for a timeout (i.e. timed-wait semantics).

Possible osStatus_t return values:

- osOK: the message has been put into the queue.
- osErrorTimeout: the message could not be put into the queue in the given time (wait-timed semantics).
- osErrorResource: not enough space in the queue (try semantics).
- osErrorParameter: parameter mq_id is NULL or invalid, non-zero timeout specified in an ISR.
- osErrorSafetyClass: the calling thread safety class is lower than the safety class of the specified message queue.

Note
  May be called from Interrupt Service Routines if the parameter timeout is set to 0.

Code Example:

#include "cmsis_os2.h" // CMSIS RTOS header file
/*----------------------------------------------------------------------------
* Message Queue creation & usage
*---------------------------------------------------------------------------*/
#define MSGQUEUE_OBJECTS 16 // number of Message Queue Objects
typedef struct { // object data type
uint8_t Buf[32];
uint8_t Idx;
} MSGQUEUE_OBJ_t;
osMessageQueueId_t mid_MsgQueue; // message queue id
osThreadId_t tid_Thread_MsgQueue1; // thread id 1
osThreadId_t tid_Thread_MsgQueue2; // thread id 2
void Thread_MsgQueue1 (void *argument); // thread function 1
void Thread_MsgQueue2 (void *argument); // thread function 2
int Init_MsgQueue (void) {
mid_MsgQueue = osMessageQueueNew(MSGQUEUE_OBJECTS, sizeof(MSGQUEUE_OBJ_t), NULL);
if (mid_MsgQueue == NULL) {
; // Message Queue object not created, handle failure
}
tid_Thread_MsgQueue1 = osThreadNew(Thread_MsgQueue1, NULL, NULL);
if (tid_Thread_MsgQueue1 == NULL) {
return(-1);
}
tid_Thread_MsgQueue2 = osThreadNew(Thread_MsgQueue2, NULL, NULL);
if (tid_Thread_MsgQueue2 == NULL) {
return(-1);
}
return(0);
}
void Thread_MsgQueue1 (void *argument) {
MSGQUEUE_OBJ_t msg;
while (1) {
; // Insert thread code here...
msg.Buf[0] = 0x55U; // do some work...
msg.Idx = 0U;
osMessageQueuePut(mid_MsgQueue, &msg, 0U, 0U);
osThreadYield(); // suspend thread
}
}
void Thread_MsgQueue2 (void *argument) {
MSGQUEUE_OBJ_t msg;
osStatus_t status;
while (1) {
; // Insert thread code here...
status = osMessageQueueGet(mid_MsgQueue, &msg, NULL, 0U); // wait for message
if (status == osOK) {
; // process data
}
}
}

## ◆ osMessageQueueGet()

osStatus_t osMessageQueueGet | ( | osMessageQueueId_t | mq_id,
|  | void * | msg_ptr,
|  | uint8_t * | msg_prio,
|  | uint32_t | timeout
| ) |  |

Get a Message from a Queue or timeout if Queue is empty.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.
  [out] | msg_ptr | pointer to buffer for message to get from a queue.
  [out] | msg_prio | pointer to buffer for message priority or NULL.
  [in] | timeout | Timeout Values or 0 in case of no time-out.

Returns
  status code that indicates the execution status of the function.

The function osMessageQueueGet retrieves a message from the message queue specified by the parameter mq_id and saves it to the buffer pointed to by the parameter msg_ptr. The message priority is stored to parameter msg_prio if not token{NULL}.

The parameter timeout specifies how long the system waits to retrieve the message from the queue. While the system waits, the thread that is calling this function is put into the BLOCKED state. The parameter timeout can have the following values:

- when timeout is 0, the function returns instantly (i.e. try semantics).
- when timeout is set to osWaitForever the function will wait for an infinite time until the message is retrieved (i.e. wait semantics).
- all other values specify a time in kernel ticks for a timeout (i.e. timed-wait semantics).

Possible osStatus_t return values:

- osOK: the message has been retrieved from the queue.
- osErrorTimeout: the message could not be retrieved from the queue in the given time (timed-wait semantics).
- osErrorResource: nothing to get from the queue (try semantics).
- osErrorParameter: parameter mq_id is NULL or invalid, non-zero timeout specified in an ISR.
- osErrorSafetyClass: the calling thread safety class is lower than the safety class of the specified message queue.

Note
  May be called from Interrupt Service Routines if the parameter timeout is set to 0.

Code Example

Refer to osMessageQueuePut

## ◆ osMessageQueueGetCapacity()

uint32_t osMessageQueueGetCapacity | ( | osMessageQueueId_t | mq_id | ) |

Get maximum number of messages in a Message Queue.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.

Returns
  maximum number of messages.

The function osMessageQueueGetCapacity returns the maximum number of messages in the message queue object specified by parameter mq_id or 0 in case of an error.

Note
  This function may be called from Interrupt Service Routines.

## ◆ osMessageQueueGetMsgSize()

uint32_t osMessageQueueGetMsgSize | ( | osMessageQueueId_t | mq_id | ) |

Get maximum message size in a Message Queue.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.

Returns
  maximum message size in bytes.

The function osMessageQueueGetMsgSize returns the maximum message size in bytes for the message queue object specified by parameter mq_id or 0 in case of an error.

Note
  This function may be called from Interrupt Service Routines.

## ◆ osMessageQueueGetCount()

uint32_t osMessageQueueGetCount | ( | osMessageQueueId_t | mq_id | ) |

Get number of queued messages in a Message Queue.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.

Returns
  number of queued messages.

The function osMessageQueueGetCount returns the number of queued messages in the message queue object specified by parameter mq_id or 0 in case of an error.

Note
  This function may be called from Interrupt Service Routines.

## ◆ osMessageQueueGetSpace()

uint32_t osMessageQueueGetSpace | ( | osMessageQueueId_t | mq_id | ) |

Get number of available slots for messages in a Message Queue.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.

Returns
  number of available slots for messages.

The function osMessageQueueGetSpace returns the number available slots for messages in the message queue object specified by parameter mq_id or 0 in case of an error.

Note
  This function may be called from Interrupt Service Routines.

## ◆ osMessageQueueReset()

osStatus_t osMessageQueueReset | ( | osMessageQueueId_t | mq_id | ) |

Reset a Message Queue to initial empty state.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.

Returns
  status code that indicates the execution status of the function.

The function osMessageQueueReset resets the message queue specified by the parameter mq_id.

Possible osStatus_t return values:

- osOK: the message queue has been rest.
- osErrorParameter: parameter mq_id is NULL or invalid.
- osErrorResource: the message queue is in an invalid state.
- osErrorISR: osMessageQueueReset cannot be called from interrupt service routines.
- osErrorSafetyClass: the calling thread safety class is lower than the safety class of the specified message queue.

Note
  This function cannot be called from Interrupt Service Routines.

## ◆ osMessageQueueDelete()

osStatus_t osMessageQueueDelete | ( | osMessageQueueId_t | mq_id | ) |

Delete a Message Queue object.

Parameters

  [in] | mq_id | message queue ID obtained by osMessageQueueNew.

Returns
  status code that indicates the execution status of the function.

The function osMessageQueueDelete deletes a message queue object specified by parameter mq_id. It releases internal memory obtained for message queue handling. After this call, the mq_id is no longer valid and cannot be used. The message queue may be created again using the function osMessageQueueNew.

Possible osStatus_t return values:

- osOK: the message queue object has been deleted.
- osErrorParameter: parameter mq_id is NULL or invalid.
- osErrorResource: the message queue is in an invalid state.
- osErrorISR: osMessageQueueDelete cannot be called from interrupt service routines.
- osErrorSafetyClass: the calling thread safety class is lower than the safety class of the specified message queue.

Note
  This function cannot be called from Interrupt Service Routines.