| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Enumerations
CAN Filter Operation Codes
CAN Interface » CAN Control Codes

Set CAN filter manipulation codes. More...

## Enumerations
enum | ARM_CAN_FILTER_OPERATION { ARM_CAN_FILTER_ID_EXACT_ADD , ARM_CAN_FILTER_ID_EXACT_REMOVE , ARM_CAN_FILTER_ID_RANGE_ADD , ARM_CAN_FILTER_ID_RANGE_REMOVE , ARM_CAN_FILTER_ID_MASKABLE_ADD , ARM_CAN_FILTER_ID_MASKABLE_REMOVE }

## Description

Set CAN filter manipulation codes.

## Enumeration Type Documentation

## ◆ ARM_CAN_FILTER_OPERATION

enum ARM_CAN_FILTER_OPERATION

ARM_CAN_FILTER_OPERATION provides the controls for setting the filter type. Refer to CAN Message Filtering for details.

Parameter for:

- ARM_CAN_ObjectSetFilter

Enumerator
ARM_CAN_FILTER_ID_EXACT_ADD | Add exact id filter.
ARM_CAN_FILTER_ID_EXACT_REMOVE | Remove exact id filter.
ARM_CAN_FILTER_ID_RANGE_ADD | Add range id filter.
ARM_CAN_FILTER_ID_RANGE_REMOVE | Remove range id filter.
ARM_CAN_FILTER_ID_MASKABLE_ADD | Add maskable id filter.
ARM_CAN_FILTER_ID_MASKABLE_REMOVE | Remove maskable id filter.