| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
SAI Companding
SAI Interface » SAI Control Codes » SAI Configuration

Defines companding. More...

## Macros
#define | ARM_SAI_COMPANDING_NONE (0UL << ARM_SAI_COMPANDING_Pos)
| No companding (default)
#define | ARM_SAI_COMPANDING_A_LAW (2UL << ARM_SAI_COMPANDING_Pos)
| A-Law companding.
#define | ARM_SAI_COMPANDING_U_LAW (3UL << ARM_SAI_COMPANDING_Pos)
| u-Law companding

## Description

Defines companding.

## Macro Definition Documentation

## ◆ ARM_SAI_COMPANDING_NONE

#define ARM_SAI_COMPANDING_NONE (0UL << ARM_SAI_COMPANDING_Pos)

No companding (default)

## ◆ ARM_SAI_COMPANDING_A_LAW

#define ARM_SAI_COMPANDING_A_LAW (2UL << ARM_SAI_COMPANDING_Pos)

A-Law companding.

## ◆ ARM_SAI_COMPANDING_U_LAW

#define ARM_SAI_COMPANDING_U_LAW (3UL << ARM_SAI_COMPANDING_Pos)

u-Law companding