CMSIS-DAP: DAP_TransferAbort

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_TransferAbort
Transfer Commands

Abort current Transfer. More...

Abort current Transfer.

The DAP_TransferAbort Command aborts the current transfer. The command can be executed while DAP_Transfer or DAP_TransferBlock command is still in progress. The command is ignored if there is no transfer in progress. The command itself has no response, however the aborted DAP_Transfer or DAP_TransferBlock command will respond with information about the actually transferred data.

DAP_TransferAbort Command:

| BYTE |
> 0x07 |
|******|